Adhesive Instructions
Castle Copings Stone adhesive is a 2 part Polyurethane adhesive that is ideally suited to the installation or replacement of coping stones on garden and parapet walls.
Simply mix all of Part A and Part B until the colour is consistent and apply with a notched trowel or by buttering the back of the coping stone.
Please allow 24 hours for curing and wear gloves when applying the adhesive.
The safety data sheet is available for download for more health and safety information.
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